List of roads to “light-up”

* Whyte Ave
* Jasper Ave
* Calgary Trail
* 104 ave
* 109 street
* 99 street
* 113 street
* 50 street
* Yellowhead hwy

Notes

* Use a logic level shifter between esp8266 board and led strips
* Use decoupling cap for power supply
* Use 1000 uF cap between power supply terminals
* Need 5V and min. 4A – double check this